; Windows USB CDC ACM Setup File
; Based on INF files which were:
;     Copyright (c) 2000 Microsoft Corporation
;     Copyright (C) 2007 Microchip Technology Inc.
; Likely to be covered by the MLPL as found at:
;    <http://msdn.microsoft.com/en-us/cc300389.aspx#MLPL>.

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%MFGNAME%
LayoutFile=layout.inf
DriverVer=03/11/2010,5.1.2600.3

[Manufacturer]
%MFGNAME%=DeviceList, NTamd64

[DestinationDirs]
DefaultDestDir=12

;---------------------------------------------------------------------
; Windows 2000/XP/Server2003/Vista/Server2008/7 - 32bit Sections

[DriverInstall.nt]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.nt
AddReg=DriverInstall.nt.AddReg

[DriverCopyFiles.nt]
usbser.sys,,,0x20

[DriverInstall.nt.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.nt.Services]
AddService=usbser, 0x00000002, DriverService.nt

[DriverService.nt]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys

;---------------------------------------------------------------------
;  Windows XP/Server2003/Vista/Server2008/7 - 64bit Sections

[DriverInstall.NTamd64]
include=mdmcpq.inf
CopyFiles=DriverCopyFiles.NTamd64
AddReg=DriverInstall.NTamd64.AddReg

[DriverCopyFiles.NTamd64]
usbser.sys,,,0x20

[DriverInstall.NTamd64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NTamd64.Services]
AddService=usbser, 0x00000002, DriverService.NTamd64

[DriverService.NTamd64]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys

;---------------------------------------------------------------------
;  Vendor and Product ID Definitions

[SourceDisksFiles]
[SourceDisksNames]
[DeviceList]
%DESCRIPTION%=DriverInstall, USB\VID_${USB_VID}&PID_${USB_PID_CDC_MSC}&MI_00, USB\VID_${USB_VID}&PID_${USB_PID_CDC_MSC}&MI_01, USB\VID_${USB_VID}&PID_${USB_PID_CDC_HID}&MI_00, USB\VID_${USB_VID}&PID_${USB_PID_CDC_HID}&MI_01, USB\VID_${USB_VID}&PID_${USB_PID_CDC}

[DeviceList.NTamd64]
%DESCRIPTION%=DriverInstall, USB\VID_${USB_VID}&PID_${USB_PID_CDC_MSC}&MI_00, USB\VID_${USB_VID}&PID_${USB_PID_CDC_MSC}&MI_01, USB\VID_${USB_VID}&PID_${USB_PID_CDC_HID}&MI_00, USB\VID_${USB_VID}&PID_${USB_PID_CDC_HID}&MI_01, USB\VID_${USB_VID}&PID_${USB_PID_CDC}

;---------------------------------------------------------------------
;  String Definitions

[Strings]
MFGFILENAME="pybcdc"
MFGNAME="MicroPython"
DESCRIPTION="Pyboard USB Comm Port"
SERVICE="USB Serial Driver"
